/*
 * (C) Copyright 2002
 * Gary Jennejohn, DENX Software Engineering, <gj@denx.de>
 *
 * See file CREDITS for list of people who contributed to this
 * project.
 *
 * This program is free software; you can redistribute it and/or
 * modify it under the terms of the GNU General Public License as
 * published by the Free Software Foundation; either version 2 of
 * the License, or (at your option) any later version.
 *
 * This program is distributed in the hope that it will be useful,
 * but WITHOUT ANY WARRANTY; without even the implied warranty of
 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 * GNU General Public License for more details.
 *
 * You should have received a copy of the GNU General Public License
 * along with this program; if not, write to the Free Software
 * Foundation, Inc., 59 Temple Place, Suite 330, Boston,
 * MA 02111-1307 USA
 */

OUTPUT_FORMAT("elf32-littlearm", "elf32-littlearm", "elf32-littlearm")
/*OUTPUT_FORMAT("elf32-arm", "elf32-arm", "elf32-arm")*/
OUTPUT_ARCH(arm)
ENTRY(_start)
SECTIONS
{
        . = 0x00000000;

        . = ALIGN(4);
	.text      :
	{
	  cpu/arm920t/start.o	(.text)
	  lib_arm/_umodsi3.o	(.text)
	  lib_generic/zlib.o	(.text)
	  lib_generic/crc32.o	(.text)
	  lib_generic/string.o	(.text)

	. = DEFINED(env_offset) ? env_offset : .;
	common/environment.o	(.ppcenv)

	  *(.text)
	}

        . = ALIGN(4);
        .rodata : { *(.rodata) }

        . = ALIGN(4);
        .data : { *(.data) }

        . = ALIGN(4);
        .got : { *(.got) }

	armboot_end_data = .;

        . = ALIGN(4);
        .bss : { *(.bss) }

	armboot_end = .;
}
